**SHERWOOD, DIAMANTE & BONITO BATH PANELS**

**FITTING INSTRUCTIONS:**

**This panel should only be fitted by a qualified installer.**

1. **Check the height from the floor to the underside of the bath rim.**
2. **Place the upper panel face down on a clean dry surface with the chamfered edge at the top.**
3. **Place the bottom plinth onto the back of the upper panel so the overall height of the 2 combined is the required height for the bath. Ensure that the height the upper panel and the plinth are set to does not include the chamfered top edge.**
4. **Now fix the bottom plinth to the upper panel from behind with at least 5 x 25mm long brass wood screws (not supplied), with 1 screw at both ends and the remaining spaced evenly along the plinth.**
5. **A batten should be secured to floor under the bath aligned with where the back of the bottom plinth will sit.**
6. **Lift the chamfered top edge of the panel under the rim of the bath and push the bottom part backwards until it contacts with the batten fitted to the floor and ease the bottom of the plinth to the floor.**

**If an end panel is required, the same procedure should be followed, with the end panel fitting behind the front panel.**

**This panel is intended to withstand normal humidity found in bathrooms however if at any point the panel or the plinth have to be cut to suit a particular bath length or height or to aid installation, then any cut surface must be re-sealed prior to installation. Failure to comply with this instruction may result in the MDF core absorbing water and the surface lifting and blistering. Any standing water should be wiped up immediately.**

**CARE INSTRUCTIONS:**

**This panel should only be cleaned with a lint free cloth and warm soapy water. Helpline number: 01452 317890.**